What is #NV?

What is Po and Mpo?

Why is leaf01 not connecting to spine02 and only connecting to spine01? Is it because the spines and leafs are connected to themselves respectively?

Why 2 cables running between spine01 and spine02 in the figure(40G) when it seems like there is just one in sheet?

Figure(40G) says current leafs have 32 ports but sheet shows just 16 ports?

I think what I see in the 40G sheet are MAC addresses. But what is it in the 1G sheets?

What is tagging?